
Data collected at the NHMFL in Tallahassee using the 45T magnet
Longitudinal resistance was measured using lockin amplifiers:

B, Voltage(X), Voltage(Y)

The resistivity is obtained by convertingL: 
resistivity(micro Ohm cm) =voltage(V)/(0.8E-4)