# FIG5
Files with data points that are required for recreating Fig. 5 (a-c)

## Fig. 5(a)
  * `SR_non-oscillatory_N.csv` with `N` replaced by `N=20,30,50,100,200,500,1000,5000,100000`
  * Column 1 contains the values of time with header `t`
  * Column 2 contains the Sx1 expectation values with header `Sx1`
  * Column 3 contains the standard error in these expectation values with header `standard error`

## Fig. 5(b)
  * `SR_oscillations_N.csv` with `N` replaced by `N=20,30,50,100,200,500,1000,5000,100000`
  * Column 1 contains the values of time with header `t`
  * Column 2 contains the Sx1 expectation values with header `Sx1`
  * Column 3 contains the standard error in these expectation values with header `standard error`

## Fig. 5(c)
  * `NP_oscillations_N.csv` with `N` replaced by `N=20,30,50,100,200,500,1000,5000,100000`
  * Column 1 contains the values of time with header `t`
  * Column 2 contains the Sx1 expectation values with header `Sx1`
  * Column 3 contains the standard error in these expectation values with header `standard error`
