Room temperature CW measurements of the sample in solid state, DTOL and D-DCM.
A standard sample of LiPc was used to calibrate the magnetic field.
The g-value of the standard is known with high precision and can be used to correct the instrument error.
