CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.6.1/conf/instr/spect/uxnmr.info
Date         : Fri Jan 31 12:43:06 2020
Release      : TopSpin 3.6.1
Installed in : /opt/topspin3.6.1
Host         : nmr950
OS           : CentOS Linux release 7.7.1908 (Core)
CPU          : Intel(R) Xeon(R) CPU E5-1620 v3 @ 3.50GHz (8 cores at 1396 MHz with Hyperthreading)
User         : nmrsu (NMR Super User)
System       : Avance III HD 950 NMR spectrometer
1H-frequency : 949.66 MHz
Description  : Avance III -HD
Location     : oxford
Bruker Order : 10211100
Configured in: nmr950:/opt/topspin3.6.1/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.93
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/05155 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x53   0x5    CD  R  0.3 REC-1  AQS RXAD/2 1000 Z130589/428 ECL 00.03
     3   0x34 0xda   0x1        X  2.3 REF-1  
     4   0x24 0x33     0        S  1.3 SGU-1  AQS SGU/3 1200 (2CH) Z117130/00644 ECL 01.03 FPGA-Vs=20131031
     5   0x26 0x33     0        S  1.3 SGU-2  AQS SGU/3 1200 (2CH) Z117130/00646 ECL 01.03 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  2.0 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345500_0021 W1345500/0021 ECL 20:
- TCP/IP address = 149.236.99.91
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 800-1000MHZ INR: W1345500/0021 ECL 20
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/2466 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/010419 ECL 50
BLA_W1345529_0242 W1345529/0242 ECL 01:
- TCP/IP address = 149.236.99.90
- Firmware VS    = 20120627
- Amplifier      = BLAX1000 E 6-405MHZ INR OUTR: W1345529/0242 ECL 01
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/5356 ECL 21
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/011446 ECL 50
LTRX Z109896/00205 ECL 01.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 950: Z109896/00205 ECL 01.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20180919
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 950: Z109896/00205 ECL 01.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/03220 ECL 05.02
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/03612 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Bruker Automatic Changer: device connected to 149.236.99.93:/dev/tty01
- Capacity: 596 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 2 s
- Sample Rail fast changer mode = no

Sample Changers at the spectrometer subnet:
-------------------------------------------------
Sample Changer 1: SampleJet
- TCP/IP address   = 149.236.99.55

Cryo Cooling Control Unit: CU5 - COOLING UNIT/5 Z159076/001
- TCP/IP address   = 149.236.99.94

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.7%/-0.0deg, reflection meter)
                PN=Z106278, SN=00207 from 20160212
    Module  2 : 2H
                PN=Z106273, SN=00207 from 20150917
    Module  3 : XBB31P 2HS
                PN=Z106274, SN=00205 from 20140711
    Module  4 : XBB31P 2HS
                PN=Z106274, SN=00019 from 20131205



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H500/100/250 E 800-1000MHZBLAX1000 E 6-405MHZ INR OUTR W1345500/0021 at TCP/IP 149.236.99.91)
SGU1 AUX  output -> input 2 of transmitter 2 (BLAX1000 E 6-405MHZ INR OUTR W1345529/0242 at TCP/IP 149.236.99.90)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H500/100/250 E 800-1000MHZBLAX1000 E 6-405MHZ INR OUTR W1345500/0021 at TCP/IP 149.236.99.91)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX1000 E 6-405MHZ INR OUTR W1345529/0242 at TCP/IP 149.236.99.90)
SGU3 AUX  output -> input 3 of transmitter 1 (BLAXH2H500/100/250 E 800-1000MHZBLAX1000 E 6-405MHZ INR OUTR W1345500/0021 at TCP/IP 149.236.99.91)
SGU4 NORM output -> input 3 of transmitter 2 (BLAX1000 E 6-405MHZ INR OUTR W1345529/0242 at TCP/IP 149.236.99.90)
SGU4 AUX  output -> input 4 of transmitter 1 (BLAXH2H500/100/250 E 800-1000MHZBLAX1000 E 6-405MHZ INR OUTR W1345500/0021 at TCP/IP 149.236.99.91)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAXH2H500/100/250 E 800-1000MHZBLAX1000 E 6-405MHZ INR OUTR W1345500/0021 at TCP/IP 149.236.99.91:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W uses blanking 7

transmitter 2 = BLAX1000 E 6-405MHZ INR OUTR W1345529/0242 at TCP/IP 149.236.99.90:
- amplifier X-1000W uses blanking 4
- amplifier X-300W uses blanking 4

transmitter 3 = BSMS/2 LOCK TRANSCEIVER 950 Z109896/00205 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


Switchbox (unknown: no outputs) routing
--------------------------------------------------------------------
transmitter 2 = BLAX1000 E 6-405MHZ INR OUTR W1345529/0242 at TCP/IP 149.236.99.90:
- amplifier X-1000W at blanking 4 can be routed to switchbox output 1 (unknown) and output 2 (unknown)


